<<< Previous | Home | Next >>>

The Open Group Base Specifications Issue 7
IEEE Std 1003.1-2008
Copyright © 2001-2008 The IEEE and The Open Group

#### NAME

> mbrtowc - convert a character to a wide-character code (restartable)

#### SYNOPSIS

> ``#include <wchar.h>
> size_t mbrtowc(wchar_t *restrict` pwc`, const char *restrict` s`,
> size_t` n`, mbstate_t *restrict` ps`);
> ``

#### DESCRIPTION

> [CX] The functionality described on this reference page is aligned with the ISO C standard. Any conflict between the requirements described here and the ISO C standard is unintentional. This volume of POSIX.1-2008 defers to the ISO C standard.

> If s is a null pointer, the mbrtowc() function shall be equivalent to the call:

>     mbrtowc(NULL, "", 1, ps)

> In this case, the values of the arguments pwc and n are ignored.

> If s is not a null pointer, the mbrtowc() function shall inspect at most n bytes beginning at the byte pointed to by s to determine the number of bytes needed to complete the next character (including any shift sequences). If the function determines that the next character is completed, it shall determine the value of the corresponding wide character and then, if pwc is not a null pointer, shall store that value in the object pointed to by pwc. If the corresponding wide character is the null wide character, the resulting state described shall be the initial conversion state.

> If ps is a null pointer, the mbrtowc() function shall use its own internal mbstate_t object, which shall be initialized at program start-up to the initial conversion state. Otherwise, the mbstate_t object pointed to by ps shall be used to completely describe the current conversion state of the associated character sequence. The implementation shall behave as if no function defined in this volume of POSIX.1-2008 calls mbrtowc().

> The behavior of this function is affected by the LC_CTYPE category of the current locale.

#### RETURN VALUE

> The mbrtowc() function shall return the first of the following that applies:

> 0
>   If the next n or fewer bytes complete the character that corresponds to the null wide character (which is the value stored).
> between 1 and n inclusive
>   If the next n or fewer bytes complete a valid character (which is the value stored); the value returned shall be the number of bytes that complete the character.
> (size_t)-2
>   If the next n bytes contribute to an incomplete but potentially valid character, and all n bytes have been processed (no value is stored). When n has at least the value of the {MB_CUR_MAX} macro, this case can only occur if s points at a sequence of redundant shift sequences (for implementations with state-dependent encodings).
> (size_t)-1
>   If an encoding error occurs, in which case the next n or fewer bytes do not contribute to a complete and valid character (no value is stored). In this case, [EILSEQ] shall be stored in errno and the conversion state is undefined.

#### ERRORS

> The mbrtowc() function shall fail if:

> [EILSEQ]
>   An invalid character sequence is detected.

> The mbrtowc() function may fail if:

> [EINVAL]
>   [CX] ps points to an object that contains an invalid conversion state.

The following sections are informative.

#### EXAMPLES

> None.

#### APPLICATION USAGE

> None.

#### RATIONALE

> None.

#### FUTURE DIRECTIONS

> None.

#### SEE ALSO

> mbsinit , mbsrtowcs

> XBD <wchar.h>

#### CHANGE HISTORY

> First released in Issue 5. Included for alignment with ISO/IEC 9899:1990/Amendment 1:1995 (E).

#### Issue 6

> The mbrtowc() prototype is updated for alignment with the ISO/IEC 9899:1999 standard.

> The following new requirements on POSIX implementations derive from alignment with the Single UNIX Specification:

> - The [EINVAL] error condition is added.

> ISO/IEC 9899:1999 standard, Technical Corrigendum 1 is incorporated.

#### Issue 7

> Austin Group Interpretation 1003.1-2001 #170 is applied.

End of informative text.

return to top of page

UNIX ® is a registered Trademark of The Open Group.
POSIX ® is a registered Trademark of The IEEE.
Copyright © 2001-2008 The IEEE and The Open Group, All Rights Reserved
[ Main Index | XBD | XSH | XCU | XRAT ]

<<< Previous | Home | Next >>>