# $FreeBSD: release/9.2.0/sys/sparc64/conf/NOTES 206451 2010-04-10 11:52:12Z marius $
#
# This file contains machine dependent kernel configuration notes.  For
# machine independent notes, look in /sys/conf/NOTES.


#####################################################################
# CPU OPTIONS

#
# You must specify at least one CPU (the one you intend to run on);
# deleting the specification for CPUs you don't need to use may make
# parts of the system run faster.
# XXX: On the Sparc64, there is only one CPU type
cpu		SUN4U


#####################################################################
# HARDWARE BUS CONFIGURATION

device		ebus
device		isa
device		pci
device		sbus
device		central
device		fhc


#####################################################################
# HARDWARE DEVICE CONFIGURATION

#
# Mandatory devices:
#

device		eeprom		# eeprom (really a front-end for the MK48Txx)
device		mk48txx		# Mostek MK48Txx clocks
device		rtc		# rtc (really a front-end for the MC146818)
device		mc146818	# Motorola MC146818 and compatible clocks
device		sbbc		# Sun BootBus controller

#
# Optional devices:
#

device		auxio		# auxiliary I/O device
device		epic		# Sun Fire V215/V245 LEDs
device		creator		# Creator, Creator3D and Elite3D framebuffers
device		machfb		# ATI Mach64 framebuffers

device		ofw_console	# Open Firmware console device
option 		OFWCONS_POLL_HZ=4 # 20 or more works best on Ultra2

# PS/2 mouse
device		psm

# Options for psm:
options 	PSM_HOOKRESUME		#hook the system resume event, useful
					#for some laptops
options 	PSM_RESETAFTERSUSPEND	#reset the device at the resume event

# The keyboard controller; it controls the keyboard and the PS/2 mouse.
device		atkbdc

# The AT keyboard
device		atkbd

# Options for atkbd:
options 	ATKBD_DFLT_KEYMAP	# specify the built-in keymap
makeoptions	ATKBD_DFLT_KEYMAP=jp.106

# `flags' for atkbd:
#       0x01    Force detection of keyboard, else we always assume a keyboard
#       0x02    Don't reset keyboard, useful for some newer ThinkPads
#	0x03	Force detection and avoid reset, might help with certain
#		dockingstations
#       0x04    Old-style (XT) keyboard support, useful for older ThinkPads

# Sun type 4/5/6 RS-232@TTL keyboard
#device		sunkbd

# Options for sunkbd:
options 	SUNKBD_EMULATE_ATKBD	# allows to use the AT keyboard maps
					# in share/syscons/keymaps, required
					# for SUNKBD_DFLT_KEYMAP and kbdmux
options 	SUNKBD_DFLT_KEYMAP	# specify the built-in keymap
makeoptions	SUNKBD_DFLT_KEYMAP=jp.106


#####################################################################
# Devices we don't want to deal with

nodevice	daemon_saver
nodevice	snake_saver
nodevice	star_saver
nodevice	bktr
nodevice	fdc
nodevice	ppc
nodevice	snd_ad1816
nodevice	snd_als4000
nodevice	snd_cmi
nodevice	snd_cs4281
nodevice	snd_csa
nodevice	snd_ds1
nodevice	snd_emu10k1
nodevice	snd_ess
nodevice	snd_fm801
nodevice	snd_gusc
nodevice	snd_ich
nodevice	snd_maestro
nodevice	snd_maestro3
nodevice	snd_mss
nodevice	snd_neomagic
nodevice	snd_sb16
nodevice	snd_sb8
nodevice	snd_sbc
nodevice	snd_solo
nodevice	snd_t4dwave
nodevice	snd_via8233
nodevice	snd_via82c686
nodevice	snd_vibes
nodevice	snd_uaudio
nodevice	aha
nodevice	bt
nodevice	wds
nodevice	ep
nodevice	ex


#####################################################################
# Options we don't want to deal with

nooption	FDC_DEBUG
nooption	COMPAT_FREEBSD4
nooption	SC_RENDER_DEBUG
nooption	SC_DEBUG_LEVEL
nooption	PPC_DEBUG
nooption	PPC_PROBE_CHIPSET
nooption	SC_NO_SUSPEND_VTYSWITCH
nooption	SC_NO_FONT_LOADING
nooption	SC_KERNEL_CONS_REV_ATTR
nooption	SC_KERNEL_CONS_ATTR
nooption	SC_NORM_REV_ATTR
nooption	SC_NORM_ATTR
nooption	SC_DFLT_FONT
nooption	SC_ALT_MOUSE_IMAGE
nooption	EXT2FS


#####################################################################
# Make options we don't want to deal with

nomakeoption	SC_DFLT_FONT
