# $FreeBSD: release/9.2.0/sys/ia64/conf/NOTES 223365 2011-06-21 12:38:40Z alc $
#
# This file contains machine dependent kernel configuration notes.  For
# machine independent notes, look in /sys/conf/NOTES.

# directive: cpu
# You must specify at least one CPU (the one you intend to run on). Deleting
# the support for CPUs you don't need to use may make parts of the system run
# faster. There's currently no special code for the different CPUs. Note also
# that the cpu declares the family. We may need to add support for specifying
# particular models.
cpu		ITANIUM
cpu		ITANIUM2

# option: COMPAT_FREEBSD32
# This option enables the support for execution of i386 (32-bit) programs on
# ia64. It is based on the ia32 emulation in the processor.
options 	COMPAT_FREEBSD32

# option: LOG2_ID_PAGE_SIZE
# Specify the log2 size of the identity (direct) mappings in regions 6 and 7
# of the virtual address space.
options 	LOG2_ID_PAGE_SIZE=27		# 128M

# option: LOG2_PAGE_SIZE
# Specify the log2 size of the page to be used for virtual memory management.
# The page size being equal to 1<<LOG2_PAGE_SIZE.
options 	LOG2_PAGE_SIZE=14		# 16K

# option: SKI
# Build support for running under the ski simulator.
options 	SKI

# option: UWX_TRACE_ENABLE
# Build the unwinder with tracing support. This option is used to debug the
# unwinder itself and the glue around it.
options 	UWX_TRACE_ENABLE

# MI options
options 	ACPI_DEBUG
options 	KSTACK_PAGES=3

device		acpi

device		agp
device		isa
device		pci

# PS/2 mouse
device		psm
hint.psm.0.at="atkbdc"
hint.psm.0.irq="12"

# Options for psm:
options 	PSM_HOOKRESUME		#hook the system resume event, useful
					#for some laptops
options 	PSM_RESETAFTERSUSPEND	#reset the device at the resume event

# The keyboard controller; it controls the keyboard and the PS/2 mouse.
device		atkbdc
hint.atkbdc.0.at="isa"
hint.atkbdc.0.port="0x060"

# The AT keyboard
device		atkbd
hint.atkbd.0.at="atkbdc"
hint.atkbd.0.irq="1"

# Options for atkbd:
options 	ATKBD_DFLT_KEYMAP	# specify the built-in keymap
makeoptions	ATKBD_DFLT_KEYMAP=jp.106

# `flags' for atkbd:
#       0x01    Force detection of keyboard, else we always assume a keyboard
#       0x02    Don't reset keyboard, useful for some newer ThinkPads
#	0x03	Force detection and avoid reset, might help with certain
#		dockingstations
#       0x04    Old-style (XT) keyboard support, useful for older ThinkPads

# Video card driver for VGA adapters.
device		vga
hint.vga.0.at="isa"

# Options for vga:
# Try the following option if the mouse pointer is not drawn correctly
# or font does not seem to be loaded properly.  May cause flicker on
# some systems.
options 	VGA_ALT_SEQACCESS

# If you can dispense with some vga driver features, you may want to
# use the following options to save some memory.
#options 	VGA_NO_FONT_LOADING	# don't save/load font
#options 	VGA_NO_MODE_CHANGE	# don't change video modes

# Older video cards may require this option for proper operation.
options 	VGA_SLOW_IOACCESS	# do byte-wide i/o's to TS and GDC regs

# The following option probably won't work with the LCD displays.
options 	VGA_WIDTH90		# support 90 column modes

# Debugging.
options 	VGA_DEBUG

# AGP debugging.
options 	AGP_DEBUG

# The following devices are not supported.
nodevice	fdc
nooption	FDC_DEBUG
